For 1990-2009 cars

### Removal Procedure

1. Remove the console assembly. Refer to Console Replacement in Instrument Panel, Gauges, and Console.
2. Remove the front seats. Refer to Seat Replacement .
3. Remove the floor carpet retainers. Refer to Carpet Retainer Replacement .
4. Remove the front shoulder belt anchor bolts from the floor pan. Refer to Seat Belt Retractor Replacement - Left Front in Seat Belts.
5. Remove the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
6. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
7. Remove the floor carpet.

### Installation Procedure

Caution: In order to avoid personal injury or vehicle damage when you repair or replace the carpet, use the same thickness and material size as the original installation. Always return the carpet to the original location.

1. Install the floor carpet.
2. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .
3. Install the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
4. Install the front shoulder belt anchor bolts to the floor pan. Refer to Seat Belt Retractor Replacement - Left Front in Seat Belts.
5. Install the floor carpet retainers. Refer to Carpet Retainer Replacement .
6. Install the front seats. Refer to Seat Replacement .
7. Install the console assembly. Refer to Console Replacement in Instrument Panel, Gauges, and Console.