For 1990-2009 cars

### Removal Procedure

Notice: To prevent equipment damage, never connect or disconnect the wiring harness connection from the EBCM with the ignition switch in the ON position.

1. Raise the front floor center console armrest.
2. Remove the two screws that retain the front floor console trim plate to the front floor console.
3. Open the front floor console cupholder.
4. Gently pull up on the front floor console trim plate to gain access to the traction control switch.
5. Disconnect the traction control switch wiring harness connector from the traction control switch.
6. Remove the traction control switch from the front floor console trim plate. To avoid damage to the front floor console trim plate, use a small flat bladed tool on the back side of the traction control switch to release the retaining clips.

### Installation Procedure

1. Install the traction control switch into front floor console trim plate by pressing into place until fully seated and retaining clips are fully engaged.
2. Connect the traction control switch wiring harness connector to the traction control switch.
3. Align the front floor console trim plate to the front floor console and carefully press the retaining clips into the correct mounting holes in the front floor console.
4. Close the front floor console cupholder.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the two screws that retain the front floor console trim plate to the front floor console.

Tighten
Tighten the two retaining screws to 2 N·m (18 lb in).

6. Close the front floor center console armrest.
7. Verify the repair. Refer to Diagnostic System Check - ABS .