For 1990-2009 cars

## Power Mirror Switch Replacement Pontiac

### Removal Procedure

1. With a flat-bladed tool, push in and lift up to disengage the retaining clips for the accessory switch plate.
2. Release the inside retaining tabs for the power mirror switch.
3. Press the power mirror switch out of the switch plate.

### Installation Procedure

1. Install the power mirror switch to the switch plate.
2. Press the power mirror switch into the switch plate until fully engaged.
3. Install the switch plate to the door trim panel. Press the switch plate into the trim panel until retaining clips are fully engaged.

## Power Mirror Switch Replacement Oldsmobile

### Removal Procedure

1. Remove the lower pull cup from the door trim panel. Refer to Armrest Pull Cup Replacement .
2. With a flat-bladed tool, push in and lift up to disengage the retaining clips for the accessory switch plate.
3. Release the inside retaining tabs for the power mirror switch.
4. Press the power mirror switch out of the switch plate.

### Installation Procedure

1. Install the power mirror switch to the switch plate.
2. Press the power mirror switch into the bezel until fully seated.
3. Install the switch plate to the door trim panel. Press the switch plate into the trim panel until the retaining clips are fully engaged.
4. Install the lower pull cup to the door trim panel. Refer to Armrest Pull Cup Replacement .