For 1990-2009 cars

#### Tools Required

J 29074-A Clutch Alignment Arbor

### Removal Procedure

1. Remove the transmission. Refer to Transmission Replacement in Manual Transmission - M86/M94 Getrag.
2. Remove the clutch cover bolts one turn at a time, until spring pressure is relieved.
3. Remove the clutch cover and the clutch disc.

### Installation Procedure

1. Align the Heavy Side of the flywheel assembly (stamped with an X), with the clutch cover Light Side (marked with paint).
2. Install the J 29074-A in order to support the clutch cover to the flywheel assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the clutch cover to flywheel bolts (1,2,3,4,5,6).

Tighten

1. Follow the tightening sequence. Tighten the bolts to 16 N·m (12 lb ft).
2. Tighten the bolts to specifications. Refer to Fastener Tightening Specifications .

4. Remove the J 29074-A .
5. Lubricate the inside diameter of the bearing with GM P/N 12345777, or equivalent.
6. Install the transmission. Refer to Transmission Replacement in Manual Transmission - M86/M94 Getrag.
7. Bleed the hydraulic system. Refer to Hydraulic Clutch Bleeding .
8. Connect the negative battery cable.