For 1990-2009 cars

### Removal Procedure

1. Remove the left sound insulator.
2. Remove the release cable (1) retainer from the lever assembly.
3. Remove the retaining nuts.
4. Remove the pedal assembly (2).

### Installation Procedure

1. Install the pedal assembly (2) to the cowl.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Reinstall the retaining nuts.

Tighten
Tighten the nuts to 30 N·m (25 lb ft).

3. Slip the accelerator cable (1) through the slot in the rod and then install the retainer in the rod, being sure that the retainer is seated.
4. Reinstall the left sound insulator.
5. Inspect for correct opening and closing positions by operating the accelerator pedal. Make sure that the throttle valve reaches a wide-open throttle position. If not, inspect for a damaged or bent bracket, lever, or other component, or for carpet under the accelerator pedal.