For 1990-2009 cars

## Front Floor Console Trim Plate Replacement Pontiac

### Removal Procedure

1. Position the gear selector to the Neutral position.
2. Release the front floor console trim plate from the front floor console, using a small flat-bladed tool.
3. Remove the front floor console trim plate by rotating 90° and guiding it over the shift handle.

### Installation Procedure

1. Position the front floor console trim plate over the gear selector knob sliding down and rotating 90°.
2. Align the front floor console trim plate retainers to the slots in the front floor console.
3. Install the front floor console trim plate, pressing into place until fully seated.
4. Reposition the gear selector to the Park position.

## Front Floor Console Trim Plate Replacement Oldsmobile

### Removal Procedure

1. Position the gear selector to the neutral position.
2. Remove the gear selector knob retainer, using a small flat-bladed tool.
3. Remove the gear selector knob, by pulling upward.
4. Release the front floor console trim plate retainers, using a flat bladed tool.
5. Remove the front floor console trim plate from the front floor console.
6. Disconnect the electrical connectors from the front floor console trim plate.

### Installation Procedure

1. Connect the electrical connectors to the front floor console trim plate.
2. Align the front floor console trim plate retainers to the slots in the front floor console.
3. Install the front floor console trim plate, pressing into place until fully seated.
4. Position the gear selector knob to the shift lever.
5. Install the gear selector knob retainer, pressing into place until fully seated.
6. Reposition the gear selector to the Park position.