For 1990-2009 cars

1. Remove the key from the ignition switch.
2. Connect the passenger yellow 2-way connector (3) located above the RH I/P Wiring Harness Junction Block.
3. Install the Connector Position Assurance (CPA (2) to the passenger yellow 2-way connector (3) located above the RH I/P Wiring Harness Junction Block.
4. Connect the driver yellow 2-way connector (1) located above the LH I/P Wiring Harness Junction Block.
5. Install the Connector Position Assurance (CPA) (2) to the driver yellow 2-way connector (1) located above the LH I/P Wiring Harness Junction Block.
6. Install the AIR BAG Fuse to the LH I/P Wiring Harness Junction Block.
7. Staying well away from both air bags, turn the ignition switch to the ON position.

7.1. | The AIR BAG warning lamp will flash seven times.

7.2. | The AIR BAG warning lamp will then turn OFF.

8. Perform the SIR Diagnostic System Check if the AIR BAG warning lamp does not operate as described.