For 1990-2009 cars

### Removal Procedure

1. Remove the right side instrument panel I/Pinsulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages, and Console.
2. Reposition the BCM aside. Refer to Body Control Module Replacement in Body Control System.
3. Disconnect the blower motor electrical connector.
4. Remove the blower motor retaining screws.
5. Remove the blower motor and fan assembly.

### Installation Procedure

1. Install the blower motor and fan assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the blower motor and fan assembly screws.

Tighten
Tighten the screws to 5 N·m (45 lb in).

3. Connect the blower motor electrical connector.
4. Install the BCM into position. Refer to Body Control Module Replacement in Body Control System.
5. Install the right side IP insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages, and Console.