For 1990-2009 cars

#### Tools Required

• | J 28467-B Universal Engine Support Fixture

• | J 36462-A Engine Support Adapter Leg Set

• | J-28467-501 Engine Support Fixture Adapters

1. Assemble theJ-28467-501 (2) to the J 28467-B cross bar (1).
2. Install the J 28467-B (1) and the J-28467-501 (2) to the fender rails.
3. Install theJ 36462-A (1) to the cross bar (2).
4. Install the support lift hook (1) to the cross bar (2).
5. Install the support hook (1) to the right engine lift hook (3).
6. Install the support hook (1) to the J 36462-A (2).
7. Install the support hook (1) to the left engine lift hook (3).
8. Raise the engine to release the pressure off of the engine mounts.