For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lamp housing for access. Refer to Rear Compartment Courtesy Lamp Replacement in Lighting Systems.
2. Look for the mounting tabs just to the right of the center access hole on the rear package shelf. Compress the tabs and slide the receiver down through the access hole.
3. Disconnect the electrical connector from the remote door lock receiver.
4. Remove the remote door lock receiver.

### Installation Procedure

1. Connect the electrical connector.
2. Install the receiver through the access hole. Snap the mounting tabs into place.
3. Install the rear compartment lamp housing. Refer to Rear Compartment Courtesy Lamp Replacement in Lighting Systems.
4. Reprogram the new receiver to transmitters. Refer to Transmitter Programming .