For 1990-2009 cars

### Removal Procedure

1. Remove the rear of the window run channel weather-strip retainer. Refer to Window Channel Replacement . Hold the weather-strip from the front door.
2. Remove the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
3. Remove the applique screw (2) from the door window frame.
4. Remove the applique (1) by sliding the front door frame applique upwards.

### Installation Procedure

1. Install the front door frame applique (1) to the front door.
2. Install the applique screw (2) to the door window frame.
3. Slide the front door frame applique downwards.
4. Install the front door outer belt sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .
5. Install the rear of the run channel weather-strip. Refer to Window Channel Replacement .