For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel I/P trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gages, and Console.

Important: Note the location of the hoses.

2. Remove the blue vacuum hose (1) and the green vacuum hose (2) from the defroster actuator.
3. Remove the defroster actuator.

3.1. | Lift the actuator lock tab.

3.2. | Slide off the actuator.

4. Remove the actuator linkage from the defroster door lever.

Squeeze the tabs on the lever in order to remove the linkage.

### Installation Procedure

1. Install the actuator linkage to the defroster door lever.
2. Slide the defroster actuator onto the mounting bracket until the tab locks.
3. Connect the blue vacuum hose and the green vacuum hose to the defroster actuator.
4. Install the instrument panel I/P trim pad. Refer to Instrument Panel Trim Pad Replacement in Instrument Panel, Gages, and Console.