For 1990-2009 cars

#### Tools Required

J 43244 Relay Puller Pliers

### Removal Procedure

1. Open the hood.
2. Remove the underhood electrical center cover.
3. Using the J 43244 , remove the horn relay (1) from underhood electrical center.

### Installation Procedure

1. Position the horn relay (1) to the underhood electrical center pressing in until fully seated.
2. Install the underhood electrical center cover.
3. Close the hood.