For 1990-2009 cars

#### Tools Required

J 37228 Seal Cutter

1. Remove the oil level indicator tube bracket bolt.
2. Remove the oil level indicator tube.
3. Remove the two oil pan to flywheel housing bolts (denoted by black triangles).
4. Remove the 24 upper oil pan bolts using a long bit 6 mm hex driver.
5. Seperate the upper oil pan from the engine block using J 37228 .
6. Remove the upper oil pan.