For 1990-2009 cars

### Removal Procedure

1. Remove the front wheelhouse panel liner. Refer to Front Fender Liner Replacement .
2. Remove the front fender sound insulator retainers (1) and (2) from the fender.
3. Remove the front fender sound insulator (3) from the vehicle.

### Installation Procedure

1. Install the front fender sound insulator (3) to the vehicle.
2. Install the front fender insulator retainers (1) and (2) to the fender.
3. Install the front wheelhouse panel liner. Refer to Front Fender Liner Replacement .