For 1990-2009 cars

### Removal Procedure

1. Remove the split/folding rear seat back. Refer to Rear Split Folding Seat Back Replacement .
2. Place the rear seat back on a surface that meets the following conditions:

• | Clean

• | Dry

• | Non-abrasive

3. Remove the center folding armrest. Refer to Rear Seat Armrest Replacement .
4. Separate the pad and the cover from the rear seat back frame. Refer to Rear Seat Back Cushion Cover Replacement .
5. Remove the cover (3) from the pad (1).

### Installation Procedure

1. Install the cover (3) onto the pad (1).
2. Install the pad and the cover onto the rear seat back frame. Refer to Rear Seat Back Cushion Cover Replacement .
3. Install the center folding armrest.
4. Install the split/folding rear seat back. Refer to Rear Split Folding Seat Back Replacement .