For 1990-2009 cars

### Removal Procedure

1. Pull the sunroof opening trim lace (3) away from the headliner (2).
2. Beginning at the joint, pull the sunroof opening trim lace (3) until the entire weatherstrip is removed.

### Installation Procedure

1. Beginning at the joint, fully seat the sunroof opening trim (3) lace into place around the sunroof opening.
2. Cut the sunroof opening trim lace (3) if necessary.