For 1990-2009 cars

## Rear Wheel Bearing and Hub Replacement Drum Brakes

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.

Notice: Do not hammer on brake drum as damage to the bearing could result.

3. Remove the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
4. Remove the hub and bearing assembly (4) from the axle (2). The top rear attaching bolt (5) and nut (1) will not clear the brake shoe (3) when removing the hub and bearing assembly. Partially remove the hub and bearing assembly prior to removing this bolt.
5. Disconnect the rear ABS wheel speed sensor wire connector.
6. Remove the hub and bearing assembly (4) from the vehicle.

### Installation Procedure

1. Connect the rear ABS wheel speed sensor wire connector.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hub and bearing assembly (4). Position the top rear attaching bolt (5) in the hub and bearing assembly prior to the installation in the axle assembly (2).

Tighten
Tighten the hub bolts to 85 N·m (62 lb ft).

3. Install the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
4. Install the tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
5. Lower the vehicle.

## Rear Wheel Bearing and Hub Replacement Disc Brakes

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle

in General Information.

2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in tires and Wheels.
3. Remove the brake rotor. Refer to Rear Brake Rotor Replacement in Disc Brakes.
4. Disconnect the parking brake cable from the parking brake lever. Refer to Parking Brake Front Cable Replacement in Park Brake.
5. Disconnect the wheel speed sensor cable.
6. Remove the wheel hub assembly bolts.
7. remove the wheel hub assembly (8) from the knuckle.
8. Remove the Torx® head bolts from the rear of the wheel hub assembly (8).
9. Remove the wheel hub assembly (8) from the backing plate (4).

### Installation Procedure

1. Install the wheel hub assembly (8) to the backing plate (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the Torx® head bolts to the rear of the wheel hub assembly (8).

Tighten
Tighten the bolts to 10 N·m (90 lb in).

3. Install the wheel hub assembly (8) to the knuckle.
4. Install the wheel hub assembly bolts

Tighten
Tighten the bolts to 85 N·m (62 lb ft).

5. Connect the wheel speed sensor cable.
6. Connect the parking brake cable to the parking brake lever. Refer to Parking Brake Front Cable Replacement in Park Brake.
7. Install the brake rotor. Refer to Rear Brake Rotor Replacement in Disc Brakes.
8. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels
9. Lower the vehicle.