For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the push-in retainers from the upper air deflector.
3. Remove the push-in retainers from the top of the front bumper fascia.
4. Slide the tabs from under the front fenders and remove the upper air deflector from the vehicle.

### Installation Procedure

1. Position the upper air deflector in the vehicle.
2. Slide the tabs back under the fenders.
3. Install the push-in retainers to the front bumper fascia.
4. Install the push-in retainers upper air deflector.
5. Close the hood.