For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Condenser Inlet to Discharge Hose Bolt | 25 N·m | 18 lb ft
A/C Condenser Outlet to Evaporator Line Bolt | 25 N·m | 18 lb ft
A/C Condenser to Radiator Bolt | 10 N·m | 89 lb in
Air Bleed Pipe Bolt | 42 N·m | 31 lb ft
Air Bleed Pipe Nut | 14 N·m | 10 lb ft
Coolant Inlet Pipe Cover Bolt | 14 N·m | 10 lb ft
Coolant Inlet Pipe to Water Pump Cover Bolt | 14 N·m | 10 lb ft
Coolant Outlet Bolt - 3.4L | 25 N·m | 18 lb ft
Cooling Fan Motor bolts | 6 N·m | 53 lb in
Fan Shroud Bolt | 10 N·m | 89 lb in
Lower Radiator Mounting Panel Bolt | 10 N·m | 89 lb in
Surge Tank Bolt | 10 N·m | 89 lb in
Transaxle Oil Cooler Fittings at Radiator | 30 N·m | 22 lb ft
Water Pump Cover to Engine Block Bolt | 26 N·m | 19 lb ft
Water Pump Cover to Water Pump Bolt | 14 N·m | 10 lb ft
Water Pump to Timing Chain Housing Nut | 26 N·m | 19 lb ft