For 1990-2009 cars

### Removal Procedure

1. Starting at the rear edge, pull the floor carpet retainers upward in order to disengage the retaining clips.
2. Remove the driver's side floor carpet retainer (1).
3. Remove the passenger's side floor carpet retainer (1).

### Installation Procedure

1. Install the driver's side floor carpet retainer (1).

Ensure the retainers lock into place.

2. Install the passenger's side floor carpet retainer (1).