For 1990-2009 cars

### Removal Procedure

1. Remove the front seat headrest. Refer to Front Seat Head Restraint Replacement .
2. Remove the front seat headrest retainers. Refer to Front Seat Head Restraint Replacement .
3. Unfasten the J-hook retainer at the bottom of the seat back cover.
4. Pull back the rear of the front seat cushion cover in order to access the loop tab on the seat back cover. Refer to Front Seat Cushion Cover Replacement .

Unhook the loop tab from the stud.

5. Pull out the front seat back cover end flaps.
6. Reach inside of the front seat back cover in order to unfasten the hook and the loop retainers securing the front seat back cover to the pad.
7. Remove the front seat back cover from the seat back, by pulling the seat back cover up and over the pad.
8. Remove the front seat back cover from the pad.

### Installation Procedure

1. Position the front seat back cover to the pad.
2. Pull the seat back cover over the pad and align the hook and the loop retainers.
3. Use firm hand pressure in order to fasten the hook and the loop retainers, securing the front seat back cover to the pad.
4. Pull back the front seat back cover end flaps.
5. Hook the loop tab to the stud.
6. Pull back the rear of the front seat cushion cover. Refer to Front Seat Cushion Cover Replacement .
7. Fasten the J-hook retainer at the bottom of the seat back cover.
8. Install the front seat headrest retainers. Refer to Front Seat Head Restraint Replacement .
9. Install the front seat headrest. Refer to Front Seat Head Restraint Replacement .