For 1990-2009 cars

### Circuit Description

The Tire Pressure Monitor (TPM) system uses the Electronic Brake Control Module (EBCM), and The ABS wheel speed sensor inputs to monitor tire pressure. The EBCM contains software to calculate relative tire pressure differences. The EBCM monitors the ABS wheel speed sensor inputs, which will all be the same as the learned calibration if the tire pressures stay the same. If the pressure increases or decreases in one tire so too will that tire's circumference and radius, which causes that wheel speed sensor input to change. The EBCM recognizes this change in wheel speed as a tire pressure condition.

### Conditions for Running the DTC

• | No ABS or TCS malfunctions present.

• | The calibration process is at least partially complete.

• | The vehicle speed is between 24-145 km/h (15-90 mph).

### Conditions for Setting the DTC

• | The EBCM detects a tire pressure difference in one tire of 69 kPa (10 psi) higher or lower than the other three.

• | A loss of, or low system battery voltage.

### Actions Taken When the DTC Sets

• | A DTC C1245 is stored in memory.

• | The IPC displays the LOW TIRE PRESSURE warning indicator.

• | The TPM system is disabled.

### Conditions for Clearing the DTC

• | A current DTC will clear when the system has been reset.

• | A history DTC will clear after 100 consecutive malfunction free ignition cycles and the system has been reset.

• | Using the scan tool

### Diagnostic Aids

Any of the following conditions can also cause this DTC to set.

• | The tire pressures have been adjusted without resetting the TPM system.

• | The tires have been rotated or replaced without resetting the TPM system.

• | Rough or slippery road conditions such as dirt, gravel, wet, snow, or ice.

• | Tires out of balance

• | A suspension out of alignment.

### Test Description

The number below refers to the step number on the diagnostic table.

1. Tests if the tires are adjusted to the recommended kPa/psi.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Tire Pressure Monitoring System Schematics
1 | Did you perform the Tire Pressure Monitor Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Tire Pressure Monitoring
2 | Inspect the tire pressures and adjust to the recommended kPa/psi if needed. Refer to Tire Inflation Pressure Specifications in Maintenance and Lubrication, or to Tire Placard in General Information. Did incorrect tire pressure cause the DTC to set? | Go to Step 3 | Go to Diagnostic Aids
3 | Reset the TPM system. Refer to Tire Pressure Monitor Procedure . Did you complete the repair? | Go to Step 4 | --
4 |

1. use the scan tool in order to clear the DTC.
2. Operate the vehicle within the conditions for running the DTC.

Does the DTC reset?

Go to Step 2

System OK