For 1990-2009 cars

Inspect the flexible hydraulic brake hoses at least twice a year. The hydraulic brake hoses transmit hydraulic pressure to the calipers from the steel brake lines on the body.

• |
- Inspect the brake hoses (1) for the following conditions:

- | Road hazard damage

- | Cracks

- | Chafing of the outer cover

- | Leaks

- | Blisters

- | Proper routing and mounting

- | Adequate inspection may require a light and a mirror.

• | If you observe any faulty conditions on a brake hose, replace the brake hose.