For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Cable Bracket Nuts | 10 N·m | 89 lb in
Accelerator Pedal Retaining Nuts | 30 N·m | 22 lb ft
Air Cleaner Duct Clamp | 5 N·m | 44 lb in
Air Cleaner Outlet Resonator Clamp | 5 N·m | 44 lb in
Air Cleaner Outlet Resonator Mounting Bolt | 10 N·m | 89 lb in
Crankshaft position (CKP) Sensor Bolts | 8 N·m | 71 lb in
Engine coolant temperature (ECT) Sensor | 10 N·m | 89 lb in
Evaporative emission (EVAP) Canister Purge Valve Mounting Bracket Nut | 8 N·m | 71 lb in
EVAP Canister Retainer Bolt | 10 N·m | 89 lb in
Exhaust Heat Shield Bolt | 2.0 N·m | 18 lb in
Exhaust Heat Shield Nut | 1.0 N·m | 9 lb in
Fuel Filler Hose Clamp | 3 N·m | 27 lb in
Fuel Filter Fitting | 27 N·m | 20 lb ft
Fuel Pipe Mounting Bolts | 6 N·m | 53 lb in
Fuel Filler Pipe Attaching Screw | 10 N·m | 89 lb ft
Fuel Rail Pipe Fittings | 10 N·m | 89 lb in
Fuel Pipe Retainer Bolts | 10 N·m | 89 lb in
Fuel Pressure Regulator Retaining Bolts | 5 N·m | 44 lb in
Fuel Rail Attaching Studs | 10 N·m | 89 lb in
Fuel Tank Retaining Strap Bolt | 35 N·m | 26 lb ft
Heated oxygen sensor (H02S) 1 | 30 N·m | 22 lb ft
HO2S 2 | 41 N·m | 30 lb ft
Ignition control module (ICM) Cover Bolts | 8 N·m | 71 lb in
ICM Screws | 4 N·m | 35 lb in
Idle Air Control (IAC) Valve | 3 N·m | 27 lb in
Ignition Coil Housing Screws | 4 N·m | 35 lb in
Knock Sensor (KS) | 25 N·m | 18 lb ft
Spark Plugs | 20 N·m | 15 lb ft
Throttle Body Attaching Bolts and Studs | 10 N·m | 89 lb in
Throttle position (TP) Sensor Mounting Screw | 2 N·m | 18 lb in
Upper Air Cleaner Cover Screws | 3 N·m | 27 lb in