For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Remove the serpentine drive belt. Refer to Drive Belt Replacement in Engine Mechanical.
3. Disconnect the sensor electrical connector.
4. Remove the attaching bolt.
5. Remove the sensor.
6. If the sensor is not being replaced, inspect the sensor for wear, cracks, or leakage.

### Installation Procedure

1. Lubricate the O-ring with clean engine oil and replace if damaged.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the camshaft position sensor.

Tighten
Tighten the retaining bolt to 10 N·m (8 lb ft).

3. Connect the sensor electrical connector.
4. Reinstall the serpentine drive belt. Refer to Drive Belt Replacement in Engine Mechanical.