For 1990-2009 cars

### Removal Procedure

Notice: In order to avoid oil pan damage and possible engine failure, insert a block of wood that spans the width of the oil pan bottom between the oil pan and the jack support.

1. Support the engine at the oil pan with a floor jack and a block of wood .
2. Remove and position cruise control module aside.
3. Remove the engine mount to engine mount bracket bolts.
4. Remove the engine mount to body nuts.
5. Remove the engine mount.

### Installation Procedure

1. Install the engine mount to the vahicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the engine mount to body nuts.
3. Install the engine mount to engine mount bracket bolts.

Tighten
Tighten the nuts to 66 N·m (49 lb ft).

Tighten
Tighten the bolts to 130 N·m (96 lb ft).

4. Install the cruise control module to bracket.
5. Remove the floor jack.