For 1990-2009 cars

### Diagnostic Aids

When the clutch pedal sticks or binds during clutch pedal travel there might be a faulty bushing or a worn or damaged release bearing.

### Test Description

The number(s) below refer to the step number(s) on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step checks for worn bushings.

3. This step checks for a faulty release bearing.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: The clutch pedal sticks or binds during clutch pedal travel.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 | Check the clutch pedal bushings for wear. Are the clutch pedal bushings worn? | Go to Step 3 | System OK
3 | Repair the clutch pedal assembly. Refer to Clutch Pedal Replacement Does the clutch work properly? | System OK | Go to Step 4
4 |

1. Remove the transmission. Refer to Transmission Replacement .
2. Check the clutch release bearing cylinder.

Is the release bearing faulty?

Go to Step 5

--

5 | Replace the clutch release bearing. Refer to Clutch Actuator Cylinder Replacement Did you find and repair the condition? | Go to Step 6 | Go to Diagnostic Aids
6 |

1. Install the transmission. Refer to Transmission Replacement .
2. Operate the system in order to verify the repair.

Did you correct the condition?

System OK

Go to Step 1