For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Seat Replacement. Refer to Front Seat Replacement - Bucket .
2. Disconnect the electrical connectors from the motor.
3. Disconnect the drive cables. Refer to Seat Horizontal and Vertical Drive Cable Replacement .
4. Drill out the rivets.
5. Remove the motors (1,2, or 3) from the mounting bracket.

### Installation Procedure

1. Install the grommet to the motor support bracket. Secure the motor to the grommet using appropriate rivets.
2. Connect the drive cables. Seat Horizontal and Vertical Drive Cable Replacement .
3. Connect the electrical connectors to the motors (1,2, or 3).
4. Install the front seat. Refer to Front Seat Replacement - Bucket .