For 1990-2009 cars

### Removal Procedure

Important: Perform the radio set up procedure for new and reinstalled radios. Refer to Radio Setup .

1. Remove the instrument panel (IP) accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gages and Console.
2. Remove the radio screws.
3. Pull the radio toward you for access to the connectors.
4. Disconnect the IP wiring harness connector and the antenna cable connector from the radio.
5. Remove the radio from the IP.

### Installation Procedure

1. Position the radio to the instrument panel (IP).
2. Connect the IP wiring harness connector and the antenna cable connector to the radio.

Important: If the radio locator tab is difficult to align to the IP locator opening, pull the radio toward you and reposition the antenna cable.

3. Align the radio locator tab to the IP locator opening. Install the radio.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the radio screws.

Tighten
Tighten the radio screws to 2 N·m (18 lb in).

5. Install the IP accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement in Instrument Panel, Gages and Console.
6. Perform the radio set up procedure for new and reinstalled radios. Refer to Radio Setup .