For 1990-2009 cars

### Removal Procedure

The one-piece formed headliner consists of a molded substrate that is covered with a foam-backed cloth facing.

1. Remove the coat hooks. Refer to Coat Hook Replacement .
2. Remove the sunshades. Refer to Sunshade Replacement .
3. Remove the sunshade anchor. Refer to Sunshade Anchor Replacement .
4. Remove the roof rail assist handle, if equipped. Refer to Front Assist Handle Replacement .
5. Remove the dome lamp (1).
6. Pull down the door weatherstrips, as required.
7. Remove the sunroof lacing, if equipped.
8. Remove the sunroof switch, if equipped. Refer to Sunroof Switch Replacement in Roof.
9. Remove the windshield side upper garnish moldings. Refer to Windshield Pillar Garnish Molding Replacement .
10. Remove the center pillar upper trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
11. Remove the rear quarter upper trim panel. Refer to Rear Quarter Upper Trim Panel Replacement .
12. Pull down of the front of the overhead console to release its clips.
13. Pull down the headliner above the left front door. Disconnect the actuator harness connector attached to the headliner.
14. Disconnect the electrical connector to the windshield rear view mirror.
15. Disconnect the wire harness connector from the body harness at the left quarter, upper trim panel.
16. Remove the rear retainers from the headliner.
17. Remove the headliner from the vehicle.

### Installation Procedure

1. Position the headliner in the vehicle.
2. Install the rear retainers to the headliner.
3. Connect the wire harness connector to the body harness and the wire harness rosebud.
4. Connect the actuator connector.
5. Connect the electrical connector to the windshield rear view mirror.
6. Install the rear quarter upper trim panel. Refer to Rear Quarter Upper Trim Panel Replacement .
7. Install the center pillar upper trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
8. Install the windshield side upper garnish moldings. Refer to Windshield Pillar Garnish Molding Replacement .
9. Push upward on of the front of the overhead console to retain its clips.
10. Install the sunroof switch if equipped. Refer to Sunroof Switch Replacement in Roof.
11. Install the sunroof lacing.
12. Install the door weatherstrips.
13. Install the dome lamp.
14. Install the roof rail assist handle. Refer to Front Assist Handle Replacement .
15. Install the sunshade anchor. Refer to Sunshade Anchor Replacement .
16. Install the sunshades. Refer to Sunshade Replacement .
17. Install the coat hooks. Refer to Coat Hook Replacement .