For 1990-2009 cars

### Removal Procedure

1. Remove the battery. Refer to Battery Replacement in Engine Electrical.
2. Remove the battery tray bolts from the battery tray.
3. Remove the battery tray from the vehicle.

### Installation Procedure

1. Position the battery tray under the retaining tab and align the drain to the drain tube.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the battery tray bolts to the battery tray.

Tighten
Tighten the battery tray bolts to 5 N·m (44 lb in).

3. Install the battery. Refer to Battery Replacement in Engine Electrical.