For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the air outlet resonator. Refer to Air Cleaner Outlet Resonator Replacement in Engine Controls-2.2L (L61).
3. Remove the accelerator and cruise control cables bracket.
4. Remove the PCV hose.
5. Remove the fuel line brackets.
6. Remove the brake booster hose/pipe from it's bracket.
7. Remove the ignition coil and module assembly.
8. Remove the ground strap.
9. Remove the camshaft cover bolts.
10. Remove the camshaft cover.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the camshaft cover and bolts.

Tighten
Tighten the camshaft cover bolts to 10 N·m (89 lb in).

2. Install the ground strap.

Tighten
Tighten the ground strap bolt to 10 N·m (89 lb in).

3. Install the ignition coil and module assembly.

Tighten
Tighten the ignition coil and module assembly bolt to 10 N·m (89 lb in).

4. Install the brake booster hose/pipe to it's bracket.
5. Install the fuel line bracket.

Tighten
Tighten the fuel line bracket bolt to 10 N·m (89 lb in).

6. Install the accelerator and cruise control cables bracket.

Tighten
Tighten the accelerator and cruise control cables bracket bolt to 10 N·m (89 lb in).

7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.