For 1990-2009 cars

### Removal Procedure

1. Remove the left sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.
2. Depress the accelerator control cable tangs (1) from the pedal lever assembly.
3. Remove the accelerator control cable from the pedal lever assembly.
4. Remove the retainers (1) from the accelerator cam splash shield .
5. Remove the accelerator cam splash shield (2).
6. Remove the cruise control cable (1), if applicable.
7. Release the accelerator control cable lug (3) from the throttle body assembly.
8. Depress the tangs on the accelerator control cable (1) while pulling the accelerator control cable through the accelerator control cable bracket (4).
9. Remove the accelerator control cable out of the bracket.
10. Remove the cable from the vehicle.

### Installation Procedure

1. Route the accelerator control cable through the accelerator control cable bracket (4).
2. Press the accelerator control cable tabs (1) into the accelerator control bracket.

Ensure the tangs expand and properly seat.

3. Install the control cable lug (3) to the throttle body cam.
4. Install the cruise control cable (1), if applicable.
5. Install the accelerator cam splash shield (2).
6. Install the retainers (1) to the accelerator cam splash shield .
7. Install the cable (1) to the pedal lever assembly. Ensure the tangs are fully expanded and seated.
8. Slip the accelerator cable through the slot in the rod of the accelerator pedal and install the retainer in the rod. Ensure the retainer is seated.
9. Ensure the cable is completely seated in the throttle cam past the retaining clips.

Important: Flexible components (hoses, wires, conduits, etc.) must not be routed within 50 mm (2.0 in) of the moving parts of the accelerator linkage outboard support unless the routing is positively controlled.

10. Inspect for the correct opening and closing positions by operating the accelerator pedal. Make sure that the throttle valve reaches wide-open throttle position. If not, inspect for damaged or a bent bracket or lever
11. Install the left sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.