For 1990-2009 cars

## Power Accessory Switch Panel Replacement Oldsmobile

### Removal Procedure

1. Remove the lower pull cup from the door trim panel. Refer to Armrest Pull Cup Replacement .
2. With a small flat-bladed tool, push in and lift up to release the retaining clips for the accessory switch plate (1).
3. Disconnect the electrical connectors from the switches.
4. Remove the accessory switch plate from the door trim panel.
5. Remove the switches from the accessory switch plate, if required.

### Installation Procedure

1. Install the switches to the accessory switch plate, if required.

Drivers side shown, passenger side similar.

2. Connect the electrical connectors to the switches.
3. Install the accessory switch plate (1) to door trim panel.

Press the accessory switch plate into the door trim panel until retaining clips are engaged.

4. Install the lower pull cup to the door trim panel. Refer to Armrest Pull Cup Replacement .

## Power Accessory Switch Panel Replacement Pontiac

### Removal Procedure

1. Push in and lift up the retaining clips (2) for the accessory switch plate (1).
2. Remove the accessory switch plate (1) from the door trim panel.
3. Disconnect the electrical connectors from power accessory switches.
4. Remove the power accessory switches from the accessory switch plate, if required.

### Installation Procedure

1. Install the power accessory switches to the accessory switch plate, if required.
2. Connect the electrical connectors to the power accessory switches.
3. Install the accessory switch plate (1) to the door trim panel.
4. Press the accessory switch plate into the door trim panel until retaining clips (2) are secured.