For 1990-2009 cars

### Removal Procedure

1. Disconnect the vehicle speed sensor (VSS) electrical connector.
2. Remove the retainer bolt.
3. Pull up on the VSS in order to remove the VSS from the transaxle.

Remove the retainer.

4. Remove the O-ring.

### Installation Procedure

1. Lubricate a new O-ring with DEXRON III transmission fluid.
2. Install the new O-ring.
3. Install the VSS retainer.

Install the vehicle speed sensor (VSS) assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the VSS retainer bolt.

Tighten
Tighten the bolt to 9 N·m (80 lb in).

5. Connect the VSS connector to the VSS.
6. Lower the vehicle.