For 1990-2009 cars

### Removal Procedure

1. Pull down on the assist handle to expose the screws.
2. Remove the access covers with a small flat-bladed tool.
3. Remove the assist handle screws (1).
4. Remove the assist handle from the vehicle.

### Installation Procedure

1. Install the assist handle to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the assist handle screws (1).

Tighten
Tighten the screws to 2.3 N·m (20 lb in).

3. Install the plastic cover pressing into place until fully seated.