For 1990-2009 cars

Table 1: | Growl Noise Particularly Noticeable at Standstill

Problem | Action
--- | ---
There is excessive back pressure in the hoses or the steering gear caused by restriction | Locate and repair the restriction.
The pressure hose is touching other parts of the vehicle. | Adjust the hose position. Do not bend the tubing by hand.

#### Growl Noise Particularly Noticeable at Standstill

Problem | Action
--- | ---
There is scoring on the pressure plates, thrust plates, or rotor | Replace the power steering pump. Refer to Power Steering Pump Replacement .
There is an excessively worn cam ring | Replace the power steering pump. Refer to Power Steering Pump Replacement .