For 1990-2009 cars

#### Special Tools

EN-48869 Front Crankshaft Seal Installer

### Removal Procedure

1. Remove the crankshaft balancer. Refer to Crankshaft Balancer Replacement .
2. Pry out the crankshaft front oil seal using a suitable tool. Use care not to damage the engine front cover or the crankshaft.
3. Inspect the crankshaft, the crankshaft balancer and the engine front cover for wear and/or damage. Replace the components as necessary.

### Installation Procedure

1. Align the EN-48869 and the crankshaft front oil seal with the engine front cover and crankshaft.
2. Install the crankshaft front oil seal using the EN-48869 and a suitable tool.
3. Install the crankshaft balancer. Refer to Crankshaft Balancer Replacement .