For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 39232 Wiper Transmission Separator

1. Remove the wiper arm assemblies from the wiper transmission assembly drive shaft. Refer to Windshield Wiper Arm Replacement .
2. Remove the air inlet grille panel assembly from the vehicle. Refer to Air Inlet Grille Panel Replacement .
3. Remove the connector from the wiper motor assembly.
4. Remove 3 screws and the wiper drive system module from the vehicle.
5. Remove the wiper transmission assembly from the wiper motor crank arm using J 39232 .
6. Remove two screws and the wiper motor assembly from the tube frame.

### Installation Procedure

#### Tools Required

J 39529 Wiper Transmission Installer

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the wiper motor assembly onto the tube frame with 2 screws.

Tighten
Tighten the screws to 10 N·m (88 lb in).

2. Install the wiper transmission assembly onto the wiper motor crank arm using the J 39529 .
3. Install the wiper drive system module onto the vehicle with 3 screws.

Tighten
Tighten the screws to 10 N·m (88 lb in).

4. Install the connector onto the wiper motor assembly.
5. Install the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .
6. Install the wiper arm assemblies onto the wiper transmission assembly drive shaft. Refer to Windshield Wiper Arm Replacement .
7. Operate the wipers and check for proper operation.