For 1990-2009 cars

### Removal Procedure

1. Remove the generator. Refer to Generator Replacement .
2. Remove the bolts from the bracket.
3. Remove the bracket.
4. Remove the lift bracket.

### Installation Procedure

1. Position the lift bracket and the bracket to the cylinder head

Important: Hold the bolts in position against the cylinder head when tightening other bracket bolts.

2. Hand tighten the bolts in sequence.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install bolts to bracket.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

4. Install the generator. Refer to Generator Replacement