For 1990-2009 cars

## Defroster Grille Replacement Pontiac

### Removal Procedure

1. Release the defroster grill retainers from the instrument panel using a small flat-bladed tool.
2. Remove the defroster grill from the instrument panel by pulling up and out.

### Installation Procedure

1. Position the defroster grill to the instrument panel.
2. Install the defroster grill to the instrument panel pressing into place until fully seated.

## Defroster Grille Replacement Oldsmobile

### Removal Procedure

1. Release the defroster grill retainers from the instrument panel using a small flat-bladed tool.
2. Remove the defroster grill from the instrument panel by pulling up and out.

### Installation Procedure

1. Position the defroster grill to the instrument panel.
2. Install the defroster grill to the instrument panel pressing into place until fully seated.