For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement .
2. Disconnect the evaporative emission (EVAP) vapor pipe from the fill limiter vent valve, and fuel sender assembly.
3. Remove the EVAP vapor pipe.

### Installation Procedure

1. Position the EVAP vapor pipe on the fuel tank
2. Connect the EVAP vapor pipe to the fill limiter vent valve, and the fuel sender assembly.
3. Install the fuel tank. Refer to Fuel Tank Replacement .