For 1990-2009 cars

Notice: When installing the positive battery cable to the starter solenoid, the inner nut on the solenoid battery terminal must be tightened before the battery cable and the other leads are installed. Failure to do so will result in the solenoid or the solenoid terminal damage.

Whenever battery cables are replaced, always be certain to use a replacement cable that is the same type and length.

Always be certain when replacing a battery cable to route it the same as the original cable.

Some positive cables have additional feed wires attached to them and some negative cables have additional ground leads attached.