For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Untie and loosen the drawstrings from the seat cushion cover.
3. Unhook the seat cover loops from the front of the seat frame.
4. Unhook the seat cover loops from the rear of the seat frame.
5. Pull back the rear seat cushion cover from the pad.
6. Reach inside of the seat cover and unfasten the hook and the loop retainers.
7. Remove the seat cushion cover from the pad.

### Installation Procedure

1. Install the seat cushion cover onto the pad.
2. Hook the seat cover loops to the rear of the seat frame.
3. Hook the seat cover loops to the front of the seat frame.
4. Adjust seat cushion cover to a desired appearance.

With firm hand pressure fasten the hook and the loop retainers.

5. Pull the draw string tight.
6. Pull the draw string through the tabs on the seat frame and tie off.
7. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .