For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

2. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
3. Disconnect the hoses from the EVAP canister.
4. Disconnect the EVAP canister retainer attaching bolt.
5. Remove the EVAP canister and the retainer.

### Installation Procedure

1. Install the rearward end of the EVAP canister retainer into the slot in the EVAP bracket. Rotate the EVAP canister to insert the top of the EVAP canister under the tab.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Reinstall the EVAP canister retainer attaching bolt.

Tighten
Tighten the EVAP canister retainer attaching bolt to 10 N·m (88 lb in).

3. Connect the hoses to the canister.

Important: When installing the EVAP canister, the canister vent hose must be routed below the fuel tank fill and vent hoses.

4. Lower the vehicle.