For 1990-2009 cars

### Removal Procedure

1. Pry the door sill trim plate upward using a flat-bladed tool.
2. Clean the adhesive tape from the door sill.

Use a 50/50 solution of isophopyl and water.

3. Clean the door sill trim plate if the unit is to be reused.

### Installation Procedure

1. Install the adhesive tape to the door sill trim plate.
2. Install the door sill trim plate.

Press the unit firmly into place.