For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the front fender liner. Refer to Front Fender Liner Replacement .
3. Rotate the drive belt tensioner counterclockwise to release the spring tension.
4. Remove the drive belt.

### Installation Procedure

1. Rotate the drive belt tensioner counterclockwise to release the spring tension.
2. Install the drive belt.
3. Install the front fender liner. Refer to Front Fender Liner Replacement .
4. Lower the vehicle.