For 1990-2009 cars

#### Tools Required

• | J 36005 Rear Crankshaft Seal Installer

• | J 36660-A Torque Angle Meter

• | J 38122-A Crankshaft Balancer Holder

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the transmission assembly. Refer to Transmission Replacement in Automatic Transaxle 4T40 - E/4T45 - E or Transmission Replacement in Manual Transmission.
3. Remove the flywheel. Refer to Engine Flywheel Replacement .
4. Remove the bolts which secure the oil pan to the crankshaft seal housing.
5. Remove the bolts which secure the seal housing to the block.
6. Remove the seal housing and gasket.

Notice: Properly support the seal housing to prevent damage to the seal during removal. Damage to the seal will result in an oil leak.

7. Support the seal housing for the seal removal using 2 wood blocks of equal thickness. With the wood blocks on a flat surface, position the seal housing and the blocks so that the transmission side of the seal housing is supported across the dowel pin and the center bolt holes on both sides of the seal opening.
8. Using a small chisel in the relief grooves on the crankshaft side of the seal housing, drive the crankshaft seal evenly out of the transmission side of the seal housing.

### Installation Procedure

1. Replace the oil pan gasket if any of the following conditions exist:

• | Cuts or nicks

• | Deformation

• | Separation from the aluminum carrier

2. Inspect the strips of silicone in the following locations:

• | Across the top of the aluminum carrier at the oil pan

• | At the cylinder block

• | At the seal housing 3 way joint

3. Repair damaged strips using Silicone Sealant GM P/N 12345739 or equivalent. Use only enough sealant in order to restore the silicone strip to its original dimension.
4. Install the seal housing.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the bolts which secure the oil pan to the seal housing.

Tighten
Tighten the oil pan to seal housing bolts to 12 N·m (106 lb in).

6. Install a new rear crankshaft seal using J 36005 .
7. Install the flywheel. Refer to Engine Flywheel Replacement .
8. Install the transmission assembly. Refer to Transmission Replacement in Automatic Transaxle 4T40 - E/4T45 - E or Transmission Replacement in Manual Transmissions.
9. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
10. Check the engine oil level.
11. Start engine.
12. Check for leaks.