For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Accelerator Cable Bracket Retaining Bolts | 13 N·m | 115 lb in
Accelerator Cable Bracket Retaining Nut | 10 N·m | 88 lb in
Accelerator Pedel Retaining Bolt | 20 N·m | 15 lb ft
Camshaft Position (CMP) Sensor Retaining Bolt | 10 N·m | 90 lb in
Crankshaft Position 7X (CKP) Sensor Bolts | 11 N·m | 8 lb ft
Crankshaft Position 24X (CKP) Sensor Bolts | 10 N·m | 7 lb ft
Engine Coolant Temperature (ECT) Sensor | 23 N·m | 17 lb ft
Engine Oil Level Switch | 22 N·m | 17 lb ft
Engine Oil Pressure Indicator Switch | 16 N·m | 12 lb ft
EVAP Canister Purge Valve Bracket | 10 N·m | 7 lb ft
EVAP Vent Valve Bracket | 6 N·m | 53 lb in
Exhaust Gas Recirculation Valve to Throttle Body Adapter Bolts | 30 N·m | 22 lb ft
Fuel Filler Pipe Attaching Screws | 10 N·m | 8 lb ft
Fuel Filler Pipe Frame Attaching Screws | 10 N·m | 8 lb ft
Fuel Filter Mounting Bolt | 20 N·m | 15 lb ft
Fuel Pressure Regulator Attaching Bolt | 8.5 N·m | 76 lb in
Fuel Pressure and Return Pipes | 17 N·m | 13 lb ft
Fuel Rail Attaching Nuts or Bolts | 10 N·m | 7 lb ft
Fuel Sender Access Panel Nut | 10 N·m | 88 lb in
Fuel Tank Filler Pipe Hose Clamp | 2.5 N·m | 22 lb in
Fuel Tank Retaining Strap Bolts | 48 N·m | 35 lb ft
Heated Oxygen Sensors | 41 N·m | 30 lb ft
Idle Air Control Valve Attaching Screws | 3 N·m | 27 lb in
Ignition Coil to Ignition Control Module Screws | 4.5 N·m | 40 lb in
Ignition Controle Module Bracket to Engine Studs and Nuts | 25 N·m | 18 lb ft
In-Pipe Fuel Filter Outlet Nut | 30 N·m | 22 lb ft
Knock Sensor | 19 N·m | 14 lb in
Manifold Absolute Pressure (MAP) Sensor Retaining Bolt | 3 N·m | 27 lb in
Secondary AIR Injection Pump Brackit Bolt | 50 N·m | 37 lb ft
Secondary AIR Injection Check Valve Brackit Nut | 10 N·m | 88 lb in
Secondary AIR Injection Check Valve Mounting Bolt | 10 N·m | 88 lb in
Secondary AIR Injection Pipe Nut | 10 N·m | 88 lb in
Secondary AIR InjectionVacuum Bleed Valve Bracket Nut | 10 N·m | 88 lb in
Spark Plugs | 27 N·m | 20 lb ft
Throttle Body Retaining Nuts or Bolts | 28 N·m | 21 lb ft
Throttle Position Sensor Screws | 2 N·m | 18 lb in
Transaxle Range Switch Attaching Bolts | 28 N·m | 20 lb ft
Upper Intake Manifold Studs or Bolts | 25 N·m | 18 lb ft